#### PRINT

Syntax:

PRINT field-argument [ switches ]

Description: Sends the printer-specific [control](control.docx) code characters specified by text in field-argument to the selected printer.

Field Value: None.

Switches: Zero or more of the following field-specific-switches.

|  |  |
| --- | --- |
| \p field-argument-1 field-argument-2 | Allows PostScript strings to be sent to the printer as native PostScript codes. PostScript commands embedded in the document are carried out in the order in which they are inserted.The y-coordinate space used for PostScript commands in as follows: The graphics origin (0,0) is in the lower-left corner of the page, and the positive directions are up and to the right. PostScript [drawing](drawing.docx) instructions take place within a [drawing](drawing.docx) rectangle. The graphics origin is translated to the lower-left corner of the [drawing](drawing.docx) rectangle.text in this switch's field-argument-1 defines the [drawing](drawing.docx) rectangle on which the subsequent PostScript instructions operate. text in this switch's field-argument-2 contains the PostScript instructions.  |